{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":12,"n_cols":5,"rows_kept":12,"merged":[[0,0,0,4],[1,0,1,4]],"flags":["formulas_cached_only"]}
["监控设备清单"]
["                                                                                                单位：元"]
["序号","设备名称","技术参数","单位","数量"]
[1,"200万红外半球","DH-IPC-HDBW5250R-Z，采用超低照度1080P(1920×1080)CMOS图像传感器，低照度效果好，图像清晰度高；支持电动变焦，镜头焦距：2.8mm～12mm；支持感兴趣区域(ROI）编码，保证有用图像质量，节省存储空间；支持三码流同时输出，ACF（活动帧率控制），支持手机监控；支持走廊模式，应用更灵活；支持智能红外，红外监控距离≥30米；支持DC12V/POE供电方式，\n","个",13]
[2,"200万红外枪及","DH-IPC-HFW5250R-VF采用超低照度1080P(1920*1080)CMOS图像传感器，镜头焦距：2.8mm～12mm；DH-IPC-HFW5250R-VF支持感兴趣区域(ROI）编码，保证有用图像质量，节省存储空间；支持手机监控；支持走廊模式，应用更灵活；支持智能红外，红外监控距离≥60米；支持宽动态，3D降噪、强光抑制、背光补偿，适用不同监控环境； ICR滤光片切换功能，实现24小时监控；支持DC12V/POE供电方式","个",3]
[3,"监控硬盘","3000G/7200RPM/128M/SAS/","块",4]
[4,"硬盘录像机","嵌入式Linux实时操作系统,视频输入32路，前置 8 个SATA接口，支持直接抽拉式安装 8 个硬盘，支持2TB、3TB、4TB、6TB硬盘，1个外置eSATA接口，4个外置USB 接口，其中3个USB2.0, 1个USB3.0（后置），2个RJ45 10/100/1000Mbps自适应以太网口，1路VGA输出；2路HDMI输出，支持双4K异源输出","台",1]
[6,"POE交换机","★24个RJ45口,★2千兆SFP,交流供电；★交换容量≥32Gbps，★包转发率≥6.6Mpps。支持8K MAC地址 ；★专用电源一块，500W专用电源一块，最大输出功率370W\n","台",1]
[7,"控制桌椅","控制用电脑桌椅","套",1]
[8,"网线","安普六类原装网线","箱",5]
[9,"施工费","监控设备安装、调试，本项目为交钥匙工程","宗",1]
[10,"合计"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}